Describe Block 17 - NFT Features here.

Previous version

Block 17 - NFT Features-V2.0

== Intro ==

We are expecting the following levels of tiling.

Image Number

GSD of last image

Pre-tile Now

Post-Recon A

Post-Recon B

Area

1-11

8cm

14cm

NA

NA

Global'ish

11-17

5cm

5cm

NA

NA

Several 100m

18-23

3.4cm

5cm

NA

NA

100x100m TAG

Check Point

23-26

2.3cm

5cm

2cm

NA

50x50m TAG

Match Point

27-29

0.6cm

5cm

2cm

1cm

25x25m TAG

General

Setup

Extra item names

A 15cm DEM for evaluation

B... and following

Z is a single maplet over the region (22cm/Q=49)

Y is the tiling bigmap (22cm/Q=116)

X is the matching maplet that provides extra "umph" to the 35cm images (22cm/Q=81 - just a touch bigger)

W is the working maplet.

We use this for all of our processing.

A is a published version and not the starting thing.

V is a small bitmap that just covers the ROI

bigmap	Q	GSD	Width	Purpose
A...	67	15cm	20m	10m radius, published to the team
B, C...	200	5cm	20m	10m radius, published to the team
V	60	5cm	6m	Just barely covers the ROI, assuming 6m radius
W	350	5cm	35m	Baseline width we use for the ROI to cover outlying regions
X	99	5cm	10m	Central reference maplet. Used to denote the middle of the object for lithos, CSPLOT, etc
Y	250	5cm	35cm	The region to tile at 14 and 5cm
Z	49	5cm	5m	Temporary maplet, used in evaluation scripts -- dynamically built.

Tiling using XXXXXY, <idY>. Iterate over XXXXX, <idA>