Block 6A - Lat/Lon Tiling V0

Description

This block is used to tile the surface when you have specific latitude/longitude values you wish to use.

Assumptions

You have an initial shape model

You have run process_fits and make_sumfiles successfully

XXX120.SEED is copied into the scripts/ directory

User inputs

<path> is the path to the working directory

Procedure

# Start in the SPC working directorycd <path>/Bennu# Create a symbolic link to the file that has the commands needed to build the input scripts# Use make_scriptT_<GSD>.seed ln -s scripts/make_scriptT_120.in make_scriptT.inls -l make_scriptT.in # show that the link points to the correct placehead make_scriptT.in # This should list the top of the file, which shows LAT/LON and the first several locations# Build the scriptsmake_scriptTls # list the INN files that were created# Run the scriptsnohup sh run_script.b &# During the run, evaluate the progressfind_nofitT # This displays if there were any problemstail -f nohup # This shows any errors tail -f *OOT # Or just select the current output file# When complete, save the resultsfind_nofitT | tee outputmkdir block6Amv *INN *OOT output block6A# Once evaluation of new landmarks is complete and they are deemed “good” remove temporary filesrm TESTFILES/*rm TESTFILES1/*