Block 6B - Bigmap Tiling Lunar

Description

This block is used to tile the surface with high-resolution, bigmap-referenced landmarks.

Procedure

For bigmaps with a Q less than 1000, use standard procedures Block 6B - Bigmap Tiling v2

For bigmaps with a Q greater than 1000, break up the bigmap into a larger number of bigmaps that are all less than Q=1000.

Example

For Q=1100, make 5 IN files

Tile03m.IN

m<center of ROI>49 490.00338 1100 1.23400 1000TIL03S1.005.025111111100

Tile03m01.IN

mTIL03S <----- Reference the above map550 5500.00338 550 1.23400 1000TIL0311.005.025111111100

Tile03m02.IN

mTIL03S1650 5500.00338 550 1.23400 1000TIL0321.005.025111111100

Etc...