F3 Test Procedure

This test procedure is organized according to the Standard Processing States.

Processing State	Activity	Diagnostic Tool	Notes
Register DS images	All images which cover the TAG site
Autoregister DS images
Correlated	Iterate	find_nofitP, logEval.sh
Correlated	Fix landmarks (align images)	Repeat these two steps until correlation achieved.
Tiled	Tile at 20cm	find_nofitT	Tile a 50m wide region centered on TAG1.
Tiled	Fix landmarks as necessary
Correlated	Iterate	find_nofitP, logEval.sh
Correlated	Fix landmarks (align images)	Repeat these two steps until correlation achieved.
Imaged	Fix landmarks (add images)	Residuals (no of images per lmrk)	Ensure that model is correlated & imaged.
Fitted	Fix landmarks (fit overlaps)	logEval.sh	Work on lmrks until overlaps are fitted. Ensure that model is correlated, imaged, & fitted.
Geometry	Run Geometry to update S/C posn/ptg
Geomtery	Iterate	find_nofitP / logEval.sh
Geometry	Fix landmarks	Repeat these two steps until correlation achieved. Ensure that model is correlated, imaged, & fitted.
Residualed	Clean landmarks	Reisduals (5, 0.001, 0.001)	fix all >> which indicate images and lmrks which have shifted beyond pixel and distance thresholds. Ensure that model is correlated, imaged, fitted, & residualed.
Re-tiled	Fill any holes with new lmrks	map_coverage	Ensure that model is correlated, imaged, fitted, geometried, & residualed.
Evaluate	CompareOBJ CompareOBJ with optimal translation and rotation	Evaluate a 20m wide region centered on TAG1.