Test 01: First Boulder

Aim and Objectives

Purpose of test: Standard procedure was not creating accurate boulders (see transit below). The boulder was fuzzy, and there was actually a depression where the boulder was located. We wanted to see if tiling by hand could achieve a better solution.

Purple is truth, green is model

Additional Objectives

This was our first attempt at tiling by hand, so we were gaining experience with special cases.

Methodology

Procedures Start with a 35cm GSD and tile by hand. Step the GSD down by about a factor of 2 until reaching a 5cm GSD.

Data

Approach and Detailed Survey images of Shape 3.7. Max image resolution was 5cm/pixel, GSD max of 5cm.

Results

We tiled at higher and higher GSD, but we were not able to get to a high enough GSD to properly represent the boulder. The image pixel size was just not high enough to support the small maplets needed to properly

represent the boulder.

Conclusions and Recommendations

If we want to accurately represent these large boulders, we will need higher resolution images. This may require additional image planning during the mission if we need to properly represent these large boulders.