Describe LOC2PIX here.

SUBROUTINE LOC2PIX(PICNM,V,UX,UY,UZ,SCALE,DPIC_DLOC)

Change in the image-space location basued upon maplet computed in the maplet frame.

* CHARACTER*12 PICNM

Image name

Passed in.

* DOUBLE PRECISION V(3)

Centeral vector to the spot you want the data

Passed in.

* DOUBLE PRECISION UX(3)

* DOUBLE PRECISION UY(3)

* DOUBLE PRECISION UZ(3)

Normal place at that spot.

Passed in.

* DOUBLE PRECISION SCALE

Scale of the maplet

Passed in.

* DOUBLE PRECISION DPIC_DLOC(2,3)

Slope at that point.

Computed in this rotune.

categorySubroutine