20 Nov 2022

Technique by APL for putting landmarks on the limb and keeping the limb points part of the densify process.

1) Get the list of limb points -- standard limber or limbers 1) Use them directly or bin them (remember to use West Longitude) 1) Create a maplet on the limb even if you don't have any images. 1) Improve the height of the maplet in LITHOS when running "find_height", option 2

awk script to rebin things

# Eric E. Palmer - 20 Nov 2022# This reads the output from latlonConvert -- (assumes E longitude# and fixes it# It builds the make_scriptT with a special that will creaet# a landmark that is only to be used for limb evaluationBEGIN { binSize=5}// { lat = int(($2+2.5)/binSize) lon = int(-1 * ($1+2.5)/binSize) val=lat "," lon gridA [val] = 1}END { print "LATLON" print "support/tile-limbs.seed" for (lat=-90; lat<=90; lat++) { for (lon=-360; lon<=360; lon++){ val=lat "," lon if ( gridA [val] == 1 ) print lat*binSize, lon*binSize } #for } print "END"}

LITHOS copy/paste find-height

# integrate243 5 72.010.025 300U1

Tile seed

0.0010, 24# Turn on auto-namingg# Load maplet- may not be needediann# Load map and savemu1# Set limbsorn3n3 5 7qEND