MMAPL1: F2 Test 10 Ultra-Feature - Lockheed Feature 1 (Crater)

Alternate Procedure

Information from lower resolution maplets IS NOT included in the evaluation DTM.

Results

CompareOBJ RMS

Processing Step	Highest Image Resolution (cm/pixel)	CompareOBJ RMS (cm)
No Translation/Rotation	With Optimal Translation and Rotation	With Manual Translation
2cm-Tiling	1.0	1.309	1.139
1cm-Tiling	1.0	1.206	1.222
0.5cm-Tiling	1.0	1.114	1.092
0.5cm-Increase Image Res	0.25	1.226	1.208
0.5cm-Iteration 1	0.25	1.259	1.241
0.5cm-Iteration 2	0.25	1.287	1.266
0.5cm-Iteration 3	0.25	1.246	1.230
0.5cm-Iteration 3	0.25	1.217	1.200

Residual RMS

Processing Step	Highest Image Resolution (cm/pixel)	Residual RMS (cm)
2cm-Tiling	1.0	0.690
1cm-Tiling	1.0	0.361
0.5cm-Tiling	1.0	0.513
0.5cm-Increase Image Res	0.25	1.005
0.5cm-Iteration 1	0.25	0.975
0.5cm-Iteration 2	0.25	0.982
0.5cm-Iteration 3	0.25	0.974
0.5cm-Iteration 3	0.25	0.968

Showmap

Images of the evaluation bigmap at various processing steps and images resolutions.

Topographic Transits

North-South transits at various pixel locations in the evaluation bigmap, compared to truth. Transits in clouded for a number of processing steps.

Heatmap

Heatmap depicting difference between evaluation bigmap and truth.

Comparison Between Standard and Alternate Procedure