MMAPL1: F2 Test 10 Ultra-Feature - Lockheed Feature 1 (Crater)

Standard Procedure

Information from lower resolution maplets IS included in the evaluation DTM.

Results

Processing Step	Highest Image Resolution (cm/pixel)	CompareOBJ RMS (cm)
No Translation/Rotation	With Optimal Translation and Rotation	With Manual Translation
2cm-Tiling	1.0	1.396	1.279
1cm-Tiling	1.0	1.167	1.189
0.5cm-Tiling	1.0	1.084	1.074
0.5cm-Increase Image Res	0.25	1.136	1.158
0.5cm-Iteration 1	0.25	1.152	1.177
0.5cm-Iteration 2	0.25	1.168	1.180
0.5cm-Iteration 3	0.25	1.169	1.178
0.5cm-Iteration 3	0.25	1.171	1.175

Residual RMS

Processing Step	Highest Image Resolution (cm/pixel)	Residual RMS (cm)
2cm-Tiling	1.0
1cm-Tiling	1.0
0.5cm-Tiling	1.0
0.5cm-Increase Image Res	0.25
0.5cm-Iteration 1	0.25
0.5cm-Iteration 2	0.25
0.5cm-Iteration 3	0.25
0.5cm-Iteration 3	0.25

Showmap

Images of the evaluation bigmap at various processing steps and images resolutions.

Topographic Transits

North-South transits at various pixel locations in the evaluation bigmap, compared to truth. Transits in clouded for a number of processing steps.

Heatmap

Heatmap depicting difference between evaluation bigmap and truth.