MMAPL5 located at -8.858 263.551

Purpose: To test if ultra-high resolution imagery (i.e. 0.5 cm resolution) will improve the solution of shape3 topography (i.e. vertical boulders) and snap the heights of boulders into place.

Data

Data was generated by Imager_mg using shape3.8 on ormacsrv1.

- Centered at the middle of TAG site one.

Image Suite: Optimal flight path, resolutions: 50cm, 20cm, 10cm, 5cm, 1cm, and 0.5cm.

Larger maplet: Spacecraft:

Sun:

Smaller maplet Spacecraft:

Sun:

Evaluation Bigmap:

Name	GSD	Q	Width
MMAPL5	0.5cm	200	2m

Results

Test Step	CompareOBJ w/o trans or rot
step02a (tile)	2.91cm
step01a (tile)	2.80cm
step0p5a (tile)	2.66cm
step0p5b (add images, b4 didn't work)	ND
step0p5c (iterate without new images)	ND
step0p5d (ran b4 on new images)	ND
step0p5e (iterate with new images)	2.71cm

5cm GSD maplets from 5cm images

2cm GSD maplets from 1cm images

1cm GSD maplets from 1cm images

0.5cm GSD maplets from 1cm images

0.5cm GSD maplets from 0.5cm images

Tiling Script:

0.000005,49giay.5nx.0250abnXXXXXXn2u1v2ea0,65,.5,.5,0,3103n0y101n0y0c.50040103n0y101n0yeo.50au10040282.01141, 2.5, 3 6yy0.025300u1v1101n0yu10040102n0y101n0yeo.5u10040282.01141, 2.5, 3 6yy0.025300u1v1101n0yu1oRECENTy1oRECENTn3y1, 3, 5 wiRECENTnnv1u1#v#4oRECENTn1qEND

Iteration Script:

# This script performs two maplet iterations in parallel mode. # It reinitializes slope and albedo.# It recomputes maplet overlaps.# It recomputes limb fits.# It recomputes central maplet vector.# Topography determination from slopes is conditioned by:# Initial topography, # Overlapping topography, # Shadowing, # Differential stereo, # Limb heghts. # Dataless area slopes are set from the shape model.## The script hides most of the screen output. In order to obtain the # full display replace H* by #H*.## Modified 2011_12_31. Header and comments added.# Modified 2014_02_26. Hide screen output added.#H*x.025## Initialize slope and albedo.##a#y#y## Begin first iteration.#040101n0yu040## Begin topo determination.#28 fill no data with shape slope2 condition with existing topo.017 condition with shadows.0251 condition with overlapping maps4 condition with limbs1, 2.5, 3 6 condition with differential stereoy0 begin integration.025150u102n0y101n0yu## Begin second iteration.#040101n0yu040## Begin topo determination.#282.017.025141, 2.5, 3 6y0.025150u102n0yH*101n0yH*u## Begin overlaps and limb fits.#oRECENTy1oRECENTn3y1, 3, 5 ## Central vector determination.#vRECENT qEND