Test11Q:

Topography with spacecraft azimuth every 45 deg, sun at 0, 20, 40, 60, 80, and 5 cm images. CompareOBJ was run with the optimal translation and rotation option. It is important to note that images with zero phase or emission angle of 80 degrees or over were excluded.

RMS values:

STEP	CompareOBJ RMS (cm)	compMapVec RMS (cm)
1	4.896	13.791
2	3.479	7.898
3	2.606	3.677
5	1.595	1.752
10	0.679	8.954
15	0.555	12.234
20	0.519	14.578
30	0.479	17.123	Auto align turned on at step 35
50	0.399	18.958
100	0.534	19.958
150	0.534	19.998
200	1.761	20.917

Traces: