SPC Test Wish List

Here are the tests that are desired to be done during Phase E

Test	Description	Priority	Effort	Customer
Action
Pole Wobble	Test the new modules that were changed in support of the Rosetta mission to support Pole Wobble. Std error.	Action	12 weeks prep + 12 weeks	SPOC
Shape 3 redo	Run Approach phase testing to see if the improved procedures performs as well as test F4	Action	8 weeks	Jackson
Update code to SPC v3.1	Incorporate the improvements that Gaskell added to SPC during the Rosetta mission. Supports pole wobble more effectively	Action	16 weeks	SPOC
Max Slope	Do a paremeter study of the impact of the MXSLP variable, currently used for 0.6	Action	4 weeks	Jackson
OLA Albedo Integration	Work out integration of albedo into OLA	Action	3 weeks	Lockheed - Lorenz
Pole and Omega on F4	Need to run the pole and omega using F4's final shape model. May need Gaskell to train	Action	3 weeks	Palmer
High
FDS Integration	Develop the procedures and run an Approach/PreSurvey test that works on the transition to landmark navigation that contains multiple sets of data being passed	High	8 weeks	FDS
Image Quality	Generate a shape model using low(er) quality images that contain PSF, blur, hot pixels and cosmic rays	High	8 weeks	AltWG
Asteroid wall	Process Lockheed's asteroid wall	High	12 weeks	Lockheed
NFT-SPC Thread Test	Generate NFT Features and use for Decent to TAG simulation	High	scope is uncertain	Lockheed - Lorenz
Enhanced Imaging	Develop requirements and imaging plan to support. Develop high resolution DTM's based upon it	High	12 weeks	SPOC
Center of Figure / Center of Mass	SPC can shift the system of coordinates. FDS needs to have the COF mapped to COM for navigation	High	14 weeks	FDS
Medium
Operations Test: Parallel processing and team	Run Preliminary Survey and Detailed Survey portions of the mission using multiple people and multiple machines	Medium	8 weeks	SPOC
Update F2/F3 with Cross Correlation	Recompute the RMS using manually process and a Normalized Cross Correlation	Medium	5 weeks	Palmer
Low
Low	2 weeks	Palmer
Must be prioritized
Dynamics test	Do an evaluation of SCOBJ and PTG with and without the use of dynamics	8 weeks	Palmer
Uncertainty test	See the effect of different amounts of uncertainty in the solution of SPC	8 weeks	Palmer
Have starting model signif different than truth	The existing Shape 4 is only 2 meters different than the Nolan model. Run a test where we greatly increase the deviation between starting and truth	12 weeks	Jackman
NavCam distortion	Put in camera distortion for the source images and see how well SPC removes it. This is more needed for NavCam	5 weeks	Jackman
Size vs. speed error	Have a model that has a systematic error so that the size of the model is off. Then use Gaskell's speed correction analysis to identify and fix a size variation	6 weeks	Palmer

Anybody want anything else?