JAXA Training Goals

Goals

Goals

Bring the students to the "SPC Training Level 2"

Provide enough training to new personal to be able to directly and substantively help an experienced person build a shape model

Provides enough background so that additional practice and instruction can occur

Provide a systematic review of key SPC concepts and techniques to aid more experienced users understand subtle, but important, SPC dependencies

It will be insufficient to fully train new personal to a level in which they could run the Hayabusa 2 encounter without support, but it will go along way to improving their confidence with the program

Specific things to learn

Be able to create landmarks and add images

Basic trouble shooting and fixing mis-registration

Perform tiling

Do iterations

Run residuals, geometry

Optional, depending on time and understanding

Register images to shape model or maps

Autoregister

Practice

Create landmarks

Try out error-injected images into the calibration test

Student Prep

Stuff to read

Gaskell's 2008

Palmer's basic write up

Software - Please load the following

XCode - Apple's main compiler for OS X. It has many libraries you need. - https://developer.apple.com/xcode/

gfortran - https://gcc.gnu.org/wiki/GFortranBinaries#MacOS

spicelib - http://naif.jpl.nasa.gov/naif/toolkit_FORTRAN.html

MacPorts - http://www.macports.org/install.php

gnuplot - Installing using MacPorts, "sudo port install gnuplot"

imagemagick Installing using MacPorts, "sudo port install ImageMagick"

GraphicConverter -- http://www.lemkesoft.de/en/products/graphicconverter/

Activities

Day 1, Monday

Introductions and facilities

NDA.doc

Check the install the software and test cases

Introduce SPC and Bob

Intro SPC Lesson_1.pdf

Show wiki

Provide documentations, unix help

Theory of SPC

Basic SPC operation

Build landmarks Lesson 2

Fixing landmarks

Landmark management

Notes from day 1

Day 2, Tuesday

Discuss training levels Training_Notes#Training_levels

Review SPC from yesterday

Make more landmarks Notes Day 2

Manual shift

Global shift

Install spc_tools and updateDisplay

Batch shift

Introduce Lat/Lon tiling

make_scriptT

find_nofitT

Show

"find" in lithos

Show register

Day 3, Wednesday

Notes for Day 3

Work with the new model

Correct landmarks that threw errors

Build the Shape model

bigmap

Define a big map

Show how to generate

Show how to display

Setup and run a Standard_iteration Block 5 - Iterate

make_scriptP

find_nofitP

bigmap part 2

coverage_p

Build maplets using a map

Overlaps

Practice

Register

Fixing landmarks

Introduce autoregister

Day 4, Thursday

Notes, Day 4

Iteration (continuation from yesterday)

Fix landmarks from the iterate

Clean up the directory using rem_script.b

Build shape model -- Call it H2-Test2-

Change the support/buildShape.sh file

Install the shape model

Add Preliminary Survey images to the shape model

Register -- done

Autoregister the new images -- see notes

Iterate over the north pole landmarks

Build shape model -- Call it H2-Test3-

Tile the TAG site at 75 cm -- see notes

Review tools and technique to describe errors

CompareOBJ

Other tools

Error analysis

residuals

Shape model evaluation criteria Processing States

Information Needed

TAG site definition

standard_build_topography_script

standard_register_script

standard_autoregister_script

tile_120cm_seed - the seed file to tile at 120cm

tile_75cm_seed - the seed file to tile at 75cm

tile_30cm_seed - the seed file to tile at 30cm

make_scriptT_120.in - the list of latitude/longitudes needed to tile at the 120 cm level

make_scriptT_075.in - the list of latitude/longitudes needed to tile at the 75 cm level

make_scriptT_030.in - the list of latitude/longitudes needed to tile at the 30 cm level

Standard Blocks