coverage

Category D	Version 3.0

Generates global coverage of what has been tiled and processed (as per landmark files)

Input - files

view_maps.in (you get this from using update_infiles.e)

Input - stdin

What type of maps to use (all, only with landmarks and/or limbs). Typically 2

Resolution (start and ending resolution).

If you are working with limbs, do you want to see that data also?

Example

~/bin/coverage.e 0. All maps 1. Maps with lmks or limbs 2. Maps with lmks 2 0,.1 n

Output

coverage_g.pgm - a global map showing what has been tiled to the specified resolution

CategoryPrograms