densifyA

Category B	Version 3.0

Description

This program is used to increase the resolution of a shape model using albedo between landmarks.

The spatial resolution of the shape model will not increase. Adding albedo information allows for a better correlation between the shape model and landmark maps, especially when creating new landmarks.

densifyA is identical to densify except that it uses albedo.

densifyA first constructs a reference surface by interpolating the surface points of a lower resolution shape model. At each point of the reference, there is a vector V0 from the model center to that point and a normal N0 to the surface. That normal is extended some distance until it pierces one or more of the ensemble of maplets, and the average A of those distances is taken to represent the piercing point on the new model's surface. The new surface vector is V = V0 + A*N0.

The picture below is a visual representation of the paragraph above.

___...-------...___ | | | |A*N0 ______|___________|_________ reference \ / \ / V0 \ /

The new surface vector V will differ from V0 more noticeably when tiling at lower resolution because there are mismatches in maplet locations simply due to the formal uncertainties of the estimation process. Therefore, we have found it better to average the maplet normals N at each point, keeping a small randomly selected set of the A as conditioning heights.

Required Files

LMRKLIST.TXT - List of all landmarks to be used

LMKFILES/ - Directory of .LMK files for each maplet

MAPFILES/ - Directory of .MAP files

SHAPEFILES/ - Directory of built shapes

Optional Files

LMRKLISTR.TXT - Specific list of landmarks desired

Output Files

SIGMA.TXT - list of sigma values associated with the shape model (found in SHAPEFILES/)

Shape file in ICQ format

Using densifyA

Although densifyA can be run interactively, the input commands are usually prearranged in a file (e.g., "tmpRun.txt") and you invoke the program from the command line like this:

~/bin/densify < tmpRun.txt

Here is an annotated sample "tmpRun.txt" file showing the input commands:

SHAPEFILES/PreviousShapeFile (input shape)2 100 1.67773 (K (power of 2), search range (km), random seed)SHAPEFILES/CurrentShapeFile (output shape)1 (more iteration).005 (fraction of points used for conditioning).025 (conditioning weight)1 (more iterations)11111111111110 (end program)

The input commands are:

line 1 - The input SHAPE file

line 2 - A multiplicative scaling factor K (usually 2), a limit (in km) specifying how far along the surface normal the program should search for a maplet, a random seed in the form of a large integer

/!\ This random seed is superseded if you enter one on the command line after you invoke densify.

line 3 - The output SHAPE file

line 4 - 1 = an iteration

line 5 - The fraction of points used for conditioning (usually .005)

line 6 - The conditioning weight

line 7 ... - 1 = an iteration (as many as you need)

last line - 0 = end program

In most cases, the maplets will cover most of the surface. Where it is not covered, the normals to the input model provide the "slopes" and the integration proceeds without any randomly chosen conditioning heights from these areas.

In some cases, such as fast flybys of small bodies, only a small fraction of the surface is visible and vast areas are unknown. In these cases, conditioning heights are also taken from the input model as well. Specify this option by using a negative value for K (usually -2).

densifyA then determines the average height along each surface normal from each reference point of the densified shape. It also determines the average maplet surface normal and the average albedo from the maplets. It produces the output SHAPEA file in the standard ICQ format with an extra column for albedo.

After it completes the commands in the file, densifyA gives these options:

0. end program 1. proceed to iteration

If you enter '0', the output shape model will be the height averaged result.

The entire script, with the output model called SHAPEX.TXT, looks like this:

densify SHAPEFILES/SHAPE1.TXT < input shape 2, 1.0, 5639 < K, search range (km), random SEED SHAPEFILES/SHAPEX.TXT < output shape 0 < end program

If you enter '1', the program prompts:

input fraction

Enter the fraction of averaged heights (and empty heights if K<0) used to condition the integration (usually '.005').

The program prompts:

input weight

Input the weight given to the conditioning heights (usually '.025').

The program produces an output SHAPE file and gives these options:

0. end program 1. more iteration 2. change weight

The interim shape can be viewed to see whether you want to change the weight given to the conditioning heights using the procedure described below. Usually, you just continue iterating or, finally, exit the program.

By tradition, usually use:

SHAPE0 for Q=64

SHAPE1 for Q=128

SHAPE2 for Q=256

SHAPE3 for Q=512

If there have been no problems after you complete this run, at the command line enter:

cp SHAPEFILES/SHAPEX.TXT SHAPEFILES/SHAPE2.TXT

After another densification, when SHAPEX.TXT is Q=512, at the command line enter:

cp SHAPEFILES/SHAPEX.TXT SHAPEFILES/SHAPE3.TXT

SHAPE.TXT is also Q=512 and you need to update that as well.

/!\ For historical reasons, some scripts change permissions on SHAPE.TXT to read only.

At the command line enter:

chmod +w SHAPE.TXT cp SHAPEFILES/SHAPEX.TXT SHAPEFILES/SHAPE.TXT

Interactive

If you want to run densifyA interactively, the initial inputs are:

the input SHAPE file

the output SHAPE file

scaling factor K (usually 2), limit (in km) , random seed (large integer)

/!\ This random seed is superseded if you enter one on the command line after you invoke densify.

densifyA will then prompt you for the remaining inputs and iterations.

(Compiled by TC)

CategoryPrograms