make_scriptR

Category B	Version 3.0

Description

This program generates the run script and .INN files required to batch register new images.

Required Files

input file :

make_script.in - Text file containing the names of the images to batch register.

seed file :

make_scriptR.seed - Text file containing the register option commands for batch registering images.

processed files :

TESTFILES/ - Directory in which to store copies of LMRK_DISPLAY.pgm (output by register) for each image.

/!\ register requires a number of directories and files. Refer to register for more information.

Output Files

make_scriptR outputs :

run_script.b - Run script for batch image registration.

.INN files - register seed file for each image.

run_script.b output :

.OOT files - Standard output from register for each image.

processed files outputs :

TESTFILES/ - A copy of LMRK_DISPLAY.pgm (output by register) is saved for each image.

NOMINALS/ - If the seed file includes the option to update the NOMINAL file, starting S/C and camera information will be updated. (This option is not typically selected).

SUMFILES/ - S/C and camera information are updated as image shifts are made.

Using make_scriptR

1. Create Input Files

Here is a sample make_script.in file (see that entry for further information):

P3T11S2H0409 P3T11S2H0410 P3T11S2H0411END

/!\ You must precede each image filename with a space.

Here is a sample make_scriptR.seed file (see that entry for further information):

s203yXSTOP1103yXSTOP0ynnq

2. Run make_scriptR

make_scriptR generates a .INN file for each image. It consists of the image filename followed by the register options contained in the make_scriptR.seed file.

Here is a sample .INN file for image P3T11S2H0409.INN :

P3T11S2H0409s 20 3 y XSTOP 1 10 3 y XSTOP 0 y n n q

make_scriptR also generates the run_script.b script, which looks like this:

rm -f P3T11S2H0409.OOT/usr/local/bin/REGISTER < P3T11S2H0409.INN > P3T11S2H0409.OOTcp TEMPFILE.pgm ./TESTFILES/P3T11S2H0409.pgmrm -f P3T11S2H0410.OOT/usr/local/bin/REGISTER < P3T11S2H0410.INN > P3T11S2H0410.OOTcp TEMPFILE.pgm ./TESTFILES/P3T11S2H0410.pgmrm -f P3T11S2H0411.OOT/usr/local/bin/REGISTER < P3T11S2H0411.INN > P3T11S2H0411.OOTcp TEMPFILE.pgm ./TESTFILES/P3T11S2H0411.pgm

3. Batch Register Images

Here is a sample command line for running run_script.b :

sh run_script.b

The register standard output for each image is captured in the .OOT files. The LMRKDISPLAY.pgm file output by register is copied and stored in TESTFILES/ once an image has been processed. You must review the .OOT files to ascertain the success of the batch image registration process.

(!) There is currently no find-nofit program for batch image registration.

(Compiled by DL)

CategoryPrograms