newover11I:

Building topography with s/c azimuth every 90deg and 5cm images.

Results Summary:

RMS Values:

STEP	CompareOBJ (cm) w/o trans	compMapVec(cm)	NOTES
step001	ND	ND	tiling at 10cm
step002	1.62	.705	tiling at 5cm (BIGMAP instead of bigmapref)
step003	1.52	.824	(BIGMAP instead of bigmapref)
step004	1.44	.891	(BIGMAP instead of bigmapref)
step005	1.41	1.77	iteration 3
step007	1.33	1.90	iteration 5
step012	1.22	2.03	iteration 10
step013	1.21	2.01
step023	1.06	2.06
step033	0.97	1.97	iteration 31
step043	1.11	2.04	iteration 36 (step38) had a hangup. Not all maplets were iterated
step053	1.23	1.95
step063	1.28	2.01
step073	1.31	1.90
step083	1.31	1.86
step093	1.32	1.76
step103	1.28	1.76	iteration 100

Trace:

JRW Results

Heat maps: Notice how N part gets better while SE part gets worse.

Iteration 41 (same FOV as REGION)

Iteration 100 (same FOV as REGION)