Test11J:

Building topography with s/c azimuth every 90deg and 5cm images.

Results Summary:

RMS Values:

STEP	COMPAREOBJ(cm)(w/ trans)	CompareOBJ (cm) w/o trans	compMapVec(cm)	NOTES
step001	4.81	27.9	ND	I made a truth using the maplet, compMapVec and CompareOBJ w/ trans are against that truth
step002	3.80	18.7
step003	ND	13.6
step005	ND	8.09	ND	Turned on auto align
step010	ND	3.07
step020	1.09	1.66	1.42