view_maps

What this program does (Makes an image of the map coverage)

Requires - files

geometry.in -- typically, this will be copied from geometry_01.in to geometry_08.in

view_maps.in

SHAPEFILES/SHAPE00.TXT -- This is a dumbed down version of the shape.

It is used when you select the shapefile outline option (4/5/6)

Input - stdin

Menu

Running VIEW_MAPS 0. All maps 1. Maps with lmks or limbs 2. Maps with lmks 3. Maps with lmks, no albedo 4. All maps + shape outline 5. Maps with lmks or limbs + shape outline 6. Maps with lmks + shape outline

It works best to just select option 5.

This will build the object as well as put a thin line depicting the base shape (as defined by SHAPE00.txt)

Output

view.jpg -- the image taken from one of the geometry.in stations.