SETUP

F3BBLOCK-1A - Clean Setup

F3BBLOCK-1B - Test Setup

TEST

20cm

F3BBLOCK-2A - Tile 20cm

F3BBLOCK-2B - Fix landmarks

F3BBLOCK-3A - Iterate*

F3BBLOCK-3B - Fix Correlation*

10cm

F3BBLOCK-4A - Tile 10cm

F3BBLOCK-4B - Fix landmarks

F3BBLOCK-5A - Iterate*

F3BBLOCK-5B - Fix Correlation*

F3BBLOCK-6 - Fix Imaged

F3BBLOCK-7 - Fix Fitted

F3BBLOCK-8 - Geometry

F3BBLOCK-9A - Iterate*

F3BBLOCK-9B - Fix Correlation*

5cm

F3BBLOCK-10A - Tile 5cm

F3BBLOCK-10B - Fix landmarks

F3BBLOCK-11A - Iterate*

F3BBLOCK-11B - Fix Correlation*

F3BBLOCK-12 - Fix Imaged

F3BBLOCK-13 - Fix Fitted

F3BBLOCK-14 - Geometry

F3BBLOCK-15A - Iterate*

F3BBLOCK-15B - Fix Correlation*

F3BBLOCK-16 - Fix Imaged (IF NECESSARY)

F3BBLOCK-17 - Fix Fitted (IF NECESSARY)

F3BBLOCK-18 - Fix Residuals**

F3BBLOCK-19A - Iterate*,**

F3BBLOCK-19B - Fix Correlation*,**

F3BBLOCK-20 - Fix Holes (Requires repeat of steps 11-19 if any holes are found)

F3BBLOCK-21 - Evaluation

* Run recursively until maplets are "correlated". See Processing States

** Run recursively until maplets are "correlated" and "residualed". See Processing States