Block 14 - Shift V2

Description

If the model has more than <criteria> of deviation from the center of figure, then shift it to be centered

Procedure

Set-up

Set the ID. This should be the current ID, not the new one (which will really just be moved)

ID=farV03echo "Shifting the model, $ID = shapeVar" | tee -a notes

Record the current offset and make a new model that will be adjusted

cd SHAPEFILESecho shape-$ID-512 | shape_info | tee -a ../notescp shape-$ID-512 shift-$ID.txtcd ..

Run the shift command.

(Comment -- Unsure if the shape needs to be installed before geometry is run) Notice, the shape model cannot have the .TXT at the end with the shift program. FDS sends the offset with the sign flipped from what the shift program will use. FDS should have a note about this along with their delivery.

murphy/usr/local/bin/shiftOffsetX OffsetY OffsetZyshift-<whatever>nygeometry201nn

Install Shape

Install the shape and review the fit to our main images

cd SHAPEFILESecho shift-$ID.txt | shape_info | tee -a ../notesrelink.sh shift-$ID.txt SHAPE.TXT | tee -a ../notescd ..evalReg.sh lsupport/theEight

Finish the Block

echo 11 | blockFinish far\

Continue the process

While this completes the block, you still need to do the following procedures to make the shape model solid

Block 5 - Iterate v2

Block 13 - BuildShape v2

(Compiled by EEP)