Block 2 - Ingest V0

(./) Copied over from working--needs to be more general.

Description

This block additionally populates the F3 orig directory's IMAGEFILES/NOMINALS/ and SUMFILES/ sub-directories with Detailed Survey image files which are consistent across sub-tests in readiness for registering Detailed Survey images.

Assumptions

You have invoked a Bourne-Again Shell (bash) on ormacsrv1.lpl.arizona.edu

You are a member of the group OREX\spc

You have set up a skeleton directory in the following format:

/SPC_Test/F3G-Nav/ ORex/ DATA/ base/ IMAGEFILES/ SHAPEFILES/ lsupport/ orig/ results/ test/

(./) Need to figure out how we will refer to these and if they should be links. I only linked this one as a sample to see!

You have completed the processing steps in Block 1 - Setup Directory V0

User inputs

testID - Name of the F3 test directory (for example, 'F3E-Limbs')

blockID - User-specified identifier for typescript textfile name (for example, 'Block-02-01-IngestImages-TestSpecific')

Procedure

1. Initial inputs

# User inputs:testID=F3G-NavblockID=Block-02-01-IngestImages-TestSpecific

2. Set-up

# Set-Upcd /SPC_Test/$testIDscriptdatepwdls -l

(./) Not sure how this will appear. Fix numbering.

## VARIANCE-F3G:

3. Populate sub-directories

# Populate base/IMAGEFILES/ with Detailed Survey test image filesrsync -ha base/F3G-IMAGEFILES/M60* base/IMAGEFILES/rsync -ha base/F3G-IMAGEFILES/P60* base/IMAGEFILES/ls -l base/IMAGEFILES/# Populate orig/NOMINALS/ with Detailed Survey MapCam image nominalsrsync -ha base/F3G-DSM-NOMINALS/M60* orig/NOMINALS/ls -l orig/NOMINALS# Populate orig/SUMFILES/ with Detailed Survey MapCam image sumfilesrsync -ha base/F3G-DSM-SUMFILES/M60* orig/SUMFILES/ls -l orig/SUMFILES

(./) should those have further subheadings on them for each section??

## END OF VARIANCE

4. Generate PICTLIST.TXT file

# Generate lsupport/PICTLIST.TXTls base/IMAGEFILES/M* | cut -d '/' -f 3 | cut -d '.' -f 1 > lsupport/PICTLIST.TXTls base/IMAGEFILES/P* | cut -d '/' -f 3 | cut -d '.' -f 1 >> lsupport/PICTLIST.TXTsed -i -e 's/^/ /' lsupport/PICTLIST.TXT echo END >> lsupport/PICTLIST.TXT## VARIANCE-F3G:# App and PS MapCam and PolyCam images and DS MapCam images # in the region-of-interest onlyawk '/M/ { print $1 }' lsupport/PICTLIST-TAG1-100mx100m.TXT > lsupport/PICTLIST.TXTawk '/P59/ { print $1 }' lsupport/PICTLIST-TAG1-100mx100m.TXT >> lsupport/PICTLIST.TXTsed -i -e 's/^/ /' lsupport/PICTLIST.TXT echo END >> lsupport/PICTLIST.TXT## END OF VARIANCEcat lsupport/PICTLIST.TXT

5. Generate list of images needing registering/autoregistering

# Generate list of images which require registering/autoregistering## VARIANCE-F3G:# DS MapCam images within the region-of-interest only.# (PolyCam imgaes not included since the perturbations differ from sub-test to sub-test.)awk '/M60/ { print $1 }' lsupport/PICTLIST-TAG1-100mx100m.TXT > lsupport/PICTLIST-forRegistering.TXTsed -i -e 's/^/ /' lsupport/PICTLIST-forRegistering.TXT echo END >> lsupport/PICTLIST-forRegistering.TXT## END OF VARIANCEcat lsupport/PICTLIST-forRegistering.TXT

6. Complete procedure

# Block Completeexit# Save block logif [ ! -d /SPC_Test/$testID/log ]; then mkdir /SPC_Test/$testID/logfimv typescript /SPC_Test/$testID/log/log-typescript-${blockID}

(Compiled by DL)

CategoryHowTos