Local Incidence

Description

This is the process to generate local incidence for each LROC NAC image. This process involves only values found in info.txt from ISIS, and a program that reads bigmaps; it ends with an ASCII image.

Procedure

Overview

Input Details

ObjLat/Lon comes from the center pixel of the bigmap

SubSolarLat/Lon come from caminfo from ISIS (we call the output info.txt).

Code to generate NewInc.out

dumpMapInc.f

Here is a wrapper to run the compiled version of dumpMapInc.f. It also creates an ISIS cube of the results. ||Incidence Wrapper ||