Normalized Cross-Correlation Evaluation - Naming Conventions

Naming conventions have been established for:

NOMINALS/SUMFILES/IMAGEFILE names

bigmap names.

NOMINALS/SUMFILES/IMAGEFILE names

There are two naming conventions used for normalized cross-correlation evaluation files:

Naming Convention 1 was used for the smaller standard normalized cross-correlation evaluation sets (most have 9 viewing conditions per set);

Naming convention 2 was used for the comprehensive standard normalized cross-correlation evaluation set (280 viewing conditions).

NAMING CONVENTION 1

Example filename: P2F6TG3E0001:

P: Camera:

P=PolyCam;

M=MapCam;

2: Version:

numeric=truth (e.g. 2);

alpha=model (e.g. B);

F6: Test Identifier;

TG: Region Identifier:

TG=TAG Site 1;

R1=Region 1;

NF<nn>=center coordinates for natural features, see matrix below;

3E: Image Resolution, see matrix below;

00: Model State ID:

00=truth - illumination conditions are NOT corrected for latitude.

XX=truth - illumination conditions ARE corrected for latitude.

01: Viewing Condition Identifier, dependent on image version, see matrix below.

Image Resolution Matrix

a	b	c	d	e	f	g	h	i	j
9	95m	90m	9.5m	9m	95cm	90cm	9.5cm	9cm	.95cm	.9cm
8	85m	80m	8.5m	8m	85cm	80cm	8.5cm	8cm	.85cm	.8cm
7	75m	70m	7.5m	7m	75cm	70cm	7.5cm	7cm	.75cm	.7cm
6	65m	60m	6.5m	6m	65cm	60cm	6.5cm	6cm	.65cm	.6cm
5	55m	50m	5.5m	5m	55cm	50cm	5.5cm	5cm	.55cm	.5cm
4	45m	40m	4.5m	4m	45cm	40cm	4.5cm	4cm	.45cm	.4cm
3	35m	30m	3.5m	3m	35cm	30cm	3.5cm	3cm	.35cm	.3cm
2	25m	20m	2.5m	2m	25cm	20cm	2.5cm	2cm	.25cm	.2cm
1	15m	10m	1.5m	1m	15cm	10cm	1.5cm	1cm	.15cm	.1cm

Viewing Conditions Matrix

Version	Viewing Condition ID	Spacecraft	Sun
Azimuth (deg)	Zenith (deg)	Azimuth (deg)	Zenith (deg)
F3 v2	0001	0	30	90	45
F3 v2	0002	90	30	90	45
F3 v2	0003	180	30	90	45
F3 v2	0004	270	30	90	45
F3 v2	0005	0	30	270	45
F3 v2	0006	90	30	270	45
F3 v2	0007	180	30	270	45
F3 v2	0008	270	30	270	45
F3 v2	0009	45	10	270	10
F3 v2	XXX1	0	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX2	90	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX3	180	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX4	270	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX5	0	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX6	90	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX7	180	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX8	270	30	Illumination conditions corrected for latitude of feature
F3 v2	XXX9	45	10	Illumination conditions corrected for latitude of feature
NF v1 or 2	0001	0	30	90	45
NF v1 or 2	0002	90	30	90	45
NF v1 or 2	0003	180	30	90	45
NF v1 or 2	0004	270	30	90	45
NF v1 or 2	0005	0	30	270	45
NF v1 or 2	0006	90	30	270	45
NF v1 or 2	0007	180	30	270	45
NF v1 or 2	0008	270	30	270	45
NF v1 or 2	0009	45	10	270	10
NF v1 or 2	XXX1	0	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX2	90	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX3	180	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX4	270	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX5	0	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX6	90	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX7	180	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX8	270	30	Illumination conditions corrected for latitude of feature
NF v1 or 2	XXX9	45	10	Illumination conditions corrected for latitude of feature
NF v3	0001	0	30	Illumination conditions corrected for latitude of feature
NF v3	0002	90	30	Illumination conditions corrected for latitude of feature
NF v3	0003	180	30	Illumination conditions corrected for latitude of feature
NF v3	0004	270	30	Illumination conditions corrected for latitude of feature
NF v3	0005	0	30	Illumination conditions corrected for latitude of feature
NF v3	0006	90	30	Illumination conditions corrected for latitude of feature
NF v3	0007	180	30	Illumination conditions corrected for latitude of feature
NF v3	0008	270	30	Illumination conditions corrected for latitude of feature
NF v3	0009	45	10	Illumination conditions corrected for latitude of feature
F6 v2 or B	0001	0	30	90	45
F6 v2 or B	0002	90	30	90	45
F6 v2 or B	0003	180	30	90	45
F6 v2 or B	0004	270	30	90	45
F6 v2 or B	0005	0	30	270	45
F6 v2 or B	0006	90	30	270	45
F6 v2 or B	0007	180	30	270	45
F6 v2 or B	0008	270	30	270	45
F6 v2 or B	0009	45	10	270	10
F6 v2/3 or B/C	XXX1	0	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX2	90	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX3	180	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX4	270	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX5	0	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX6	90	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX7	180	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX8	270	30	Illumination conditions corrected for latitude of feature
F6 v2/3 or B/C	XXX9	45	10	Illumination conditions corrected for latitude of feature
F6 v1 or A	0001	0	30	90	20
F6 v1 or A	0002	90	30	90	20
F6 v1 or A	0003	180	30	90	20
F6 v1 or A	0004	270	30	90	20
F6 v1 or A	0005	0	30	270	20
F6 v1 or A	0006	90	30	270	20
F6 v1 or A	0007	180	30	270	20
F6 v1 or A	0008	270	30	270	20
F6 v1 or A	0009	45	10	270	10
F6 v1 or A	0010	0	30	90	30
F6 v1 or A	0011	90	30	90	30
F6 v1 or A	0012	180	30	90	30
F6 v1 or A	0013	270	30	90	30
F6 v1 or A	0014	0	30	90	50
F6 v1 or A	0015	90	30	90	50
F6 v1 or A	0016	180	30	90	50
F6 v1 or A	0017	270	30	90	50

Natural Feature Identifier Matrix

NF Id	NFT identifier	latitude (degs)	East longitude (degs)	Comments
Natural Feature 01	010012	40.0582	154.921
Natural Feature 02	010014	44.6966	162.348
Natural Feature 03	010037	47.8895	149.881
Natural Feature 04	010136	-7.90192	133.513
Natural Feature 05	010138	-1.99487	137.9
Natural Feature 06	040082	29.2658	128.917
Natural Feature 07	040293	2.77065	105.733
Natural Feature 08	070061	40.8393	118.679
Natural Feature 09	070119	43.3545	89.7089
Natural Feature 10	070266	26.8713	112.628
Natural Feature 11	070846	-9.81576	101.895
Natural Feature 12	070848	-8.10221	106.108
Natural Feature 13	090069	8.87382	92.2958
Natural Feature 14	090302	32.3793	86.8103
Natural Feature 15	090433	0.872091	66.4328
Natural Feature 16	090467	-25.6376	63.8101
Natural Feature 17	090598	-34.6589	60.6714
Natural Feature 18	110186	-36.6192	71.2703
Natural Feature 19	110216	-20.1259	64.0783
Natural Feature 20	110225	-31.8712	65.1051
Natural Feature 21	110257	-29.9054	58.0987
Natural Feature 22	110303	6.7186	74.2474
Natural Feature 23	A2	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 24	A4	-16.38544999	10.9590178	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 25	A7	-4.11341	8.41967	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 26	B7	-8.0224	16.0484	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 27	C2	-13.62341288	4.4121744	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 28	C3	-4.532795493	4.6908467	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 29	C7	-12.9103	16.4312	Note that the image is not centered on the feature, see the associated README for further details.
Natural Feature 30	C8	-3.72769	13.5271	Note that the image is not centered on the feature, see the associated README for further details.

Source MAPs

F6 Truth Images:

v2 images generated from 5cm Zmaps

v3 images generated from 1cm Zmaps

NF Truth Images:

v1 images generated from 1cm Zmaps

v2 images generated from 5cm Zmaps

Pages_file: Evaluation DIRTYSUMFILES Name Mapping.numbers.zip

NAMING CONVENTION 2

Example filename: T4A00-N-45-E:

T4: Model ID:

T4 = Truth, Shape 4;

A: Version;

00: S/C zenith (deg);

N: S/C azimuth:

Ordinal: N, E, S, W;

45: Sun zenith (deg);

E: Sun azimuth:

Ordinal: N, E, S, W.

Bigmap Names

Example bigmap name: MTG105

M: Originating shape, M=Model, T=Truth;

TG: Region Identifier, TG=TAG Site 1, R1=Region 1;

10: Ground Sample Distance (cm);

5: Width Identifier, 1=100m, 5=50m, 2=20m.

Pages_file: Evaluation DIRTYSUMFILES Name Mapping.numbers.zip

Delivered images

P1F6TG1D0001 to P1F6TG1D0009: 120cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. along)
P1F6TG7E0001 to P1F6TG7E0009: 75cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
P1F6TG3E0001 to P1F6TG3E0009: 35cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
P1F6TG2F0001 to P1F6TG2F0009: 18cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
P1F6TG9H0001 to P1F6TG9H0009: 9cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
P1F6TG5H0001 to P1F6TG5H0009: 5cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
P1F6R11D0001 to P1F6R11D0009: 120cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1F6R17E0001 to P1F6R17E0009: 75cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1F6R13E0001 to P1F6R13E0009: 35cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1F6R12F0001 to P1F6R12F0009: 18cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1F6R19H0001 to P1F6R19H0009: 9cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1F6R15H0001 to P1F6R15H0009: 5cm resolution PolyCam images centered on Rough Region 1 (45, 60, lat. elong)
P1XXTG1F0010: 10cm resolution nadir PolyCam images centered on TAG site 1 (-10, 10, lat. elong)
T4A00-N-01-E to T4A60-W-60-W: 18cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong)

Added for SPC/NFT feature evaluation (DLambert 01/19/17):
X2F6TG120001 to X2F6TG120009: 12cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 1cm Zmaps
X2F6TG1F0001 to X2F6TG1F0009: 10cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 1cm Zmaps
X2F6TG8H0001 to X2F6TG8H0009: 8cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 1cm Zmaps
P2F6TG3F0001 to P2F6TG3F0009: 30cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 5cm Zmaps
P2F6TG160001 to P2F6TG160009: 16cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 5cm Zmaps
P2F6TG120001 to P2F6TG120009: 12cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 5cm Zmaps
P2F6TG8H0001 to P2F6TG8H0009: 8cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - generated using 5cm Zmaps

Added for SPC/NFT feature evaluation (DLambert 02/03/17):
P1NF013F0001 to P1NF013F0009: 30cm resolution PolyCam images centered on natural feature 01 - generated using 1cm Zmaps
...
P1NF223F0001 to P1NF223F0009: 30cm resolution PolyCam images centered on natural feature 22 - generated using 1cm Zmaps
P1NF01160001 to P1NF01160009: 16cm resolution PolyCam images centered on natural feature 01 - generated using 1cm Zmaps
...
P1NF22160001 to P1NF22160009: 16cm resolution PolyCam images centered on natural feature 22 - generated using 1cm Zmaps
P1NF01120001 to P1NF01120009: 12cm resolution PolyCam images centered on natural feature 01 - generated using 1cm Zmaps
...
P1NF22120001 to P1NF22120009: 12cm resolution PolyCam images centered on natural feature 22 - generated using 1cm Zmaps
P1NF018H0001 to P1NF018H0009: 8cm resolution PolyCam images centered on natural feature 01 - generated using 1cm Zmaps
...
P1NF228H0001 to P1NF228H0009: 8cm resolution PolyCam images centered on natural feature 22 - generated using 1cm Zmaps
P2NF013F0001 to P2NF013F0009: 30cm resolution PolyCam images centered on natural feature 01 - generated using 5cm Zmaps
...
P2NF223F0001 to P2NF223F0009: 30cm resolution PolyCam images centered on natural feature 22 - generated using 5cm Zmaps
P2NF01160001 to P2NF01160009: 16cm resolution PolyCam images centered on natural feature 01 - generated using 5cm Zmaps
...
P2NF22160001 to P2NF22160009: 16cm resolution PolyCam images centered on natural feature 22 - generated using 5cm Zmaps
P2NF01120001 to P2NF01120009: 12cm resolution PolyCam images centered on natural feature 01 - generated using 5cm Zmaps
...
P2NF22120001 to P2NF22120009: 12cm resolution PolyCam images centered on natural feature 22 - generated using 5cm Zmaps
P2NF018H0001 to P2NF018H0009: 8cm resolution PolyCam images centered on natural feature 01 - generated using 5cm Zmaps
...
P2NF228H0001 to P2NF228H0009: 8cm resolution PolyCam images centered on natural feature 22 - generated using 5cm Zmaps

Added for SPC/NFT feature evaluation (DLambert 03/01/17):
P1NF018HXXX1 to P1NF018HXXX9: 8cm resolution PolyCam images centered on natural feature 01 - generated using 1cm Zmaps - Sun conditions corrected for feature latitude
...
P1NF228HXXX1 to P1NF228HXXX9: 8cm resolution PolyCam images centered on natural feature 22 - generated using 1cm Zmaps - Sun conditions corrected for feature latitude

P2NF018HXXX1 to P2NF018HXXX9: 8cm resolution PolyCam images centered on natural feature 01 - generated using 5cm Zmaps - Sun conditions corrected for feature latitude
...
P2NF228HXXX1 to P2NF228HXXX9: 8cm resolution PolyCam images centered on natural feature 22 - generated using 5cm Zmaps - Sun conditions corrected for feature latitude

Added for reevaluation of Shape 3 TAG site 1 with illumination conditions corrected for latitude (DLambert 03/07/17):
P2F3TG8HXXX1 to P2F3TG8HXXX9: 8cm resolution PolyCam images centered on TAG Site 1, illumination conditions corrected for latitude

Added for reevaluation of Shape 4 TAG site 1 with illumination conditions corrected for latitude (DLambert 03/07/17):
P2F6TG8HXXX1 to P2F6TG8HXXX9: 8cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - illumination conditions corrected for latitude - generated using 5cm Zmaps
P3F6TG8HXXX1 to P3F6TG8HXXX9: 8cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - illumination conditions corrected for latitude - generated using 1cm Zmaps

Added for reevaluation of Shape 4 TAG site 1 with illumination conditions corrected for latitude (DLambert 03/16/17):
P2F6TG5HXXX1 to P2F6TG5HXXX9: 5cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - illumination conditions corrected for latitude - generated using 5cm Zmaps
P3F6TG5HXXX1 to P3F6TG5HXXX9: 5cm resolution PolyCam images centered on TAG site 1 (-10, 10, lat. elong) - illumination conditions corrected for latitude - generated using 1cm Zmaps

Added for SPC/NFT feature evaluation (DLambert 04/14/17):
P3NF235H0001 to P3NF235H0009: 5cm resolution PolyCam images containing natural feature 23 - generated using 1cm Zmaps, with illumination conditions corrected for latitude
... ...
P3NF305H0001 to P3NF305H0009: 5cm resolution PolyCam images containing natural feature 30 - generated using 1cm Zmaps, with illumination conditions corrected for latitude