Current System Configuration

spc-legacy - used for processing (shall be moved)

Version: 3.0A2

ormacsrv2 - used for testing

Version: 3.0.2

ormacsrv1 - Data transfer

Planned System Configuration

ormacsrv1 - Used only for data transfer.

No processing or tools available.

spc1 - High end

spc2 - High end

spc3 - High end

spc-test - Medium end.

Used to run new versions of the software and OPIEs, SOPIEs, etc on it.

This can be old ormacsrv2.

spc-legacy - The old server that supports software version 3.0A2.

Needed for backwards compatibility of the test software (i.e. most of our test data doesn't follow the "new" and improved SIS and cannot be run).

This will be the old ormacsrv1.

Standard Configuration

File system should be case insensitive.

The directory structure:

/opt/local/spc -- the SPC-support directory.

This includes programs, scripts and support files that is needed by the SPC team.

/usr/local/bin -- The executable SPC code

/usr/local/src -- The source SPC code

/export/altwg -- The AltWG tools, managed by AltWG (Ray E.)

/Volumes/active -- The main working directory.

This should be hosted on spc1, and shared via NFT mount (or whatever allows spc1, spc2, and spc3 system to use).

The required software

ImageMagick - Installed in /opt/local/bin

SPC <version>

Altwg tools (done by AltWG and hosted on their /export/altwg)

Webserver with SPC-GUI-tools

gnuplot

GraphicsConverter

Groups Needed

OREX/spc - Limited group to only those that will run/change the active SPC model

OREX/altwg - Broad group that includes all of the AltWG

Current Hardware

As of Aug 2017

ormacsrv1

Unknown

spc-legacy

Hardware:

2x6-Core Intel Xeon 2.93GZh, 64GB

System 10.12.6

SPC version 3.0.2

ormacsrv2

Hardware:

2x6-Core Intel Xeon 2.93GZh, 64GB

System 10.12.6

SPC version 3.0.1

Cloud9

Hardware:

12-Core Intel Xeon E5, 2.7 GHz, 64GB

Mac Pro (12 core)

System ?

SPC version 3.0B5

Cloud (at PSI) -

Hardware:

12-Core Intel Xeon E5, 2.7 GHz, 16GB

Mac Pro (12 core)

System 10.12.5

SPC version 3.0A2