Describe SPC_V_and_V_testing here.

Test Info

Here is where we are putting the details of the test

F2 - Calibration Tests

Test01 - FirstBoulder - John, Tanner, Kris

Test02 - BouldersDetail - John

Test03 - ControlledCalibrationTest -- Simple peak on a flat surface - Eric

Test04 - CalibrationF2-Approach, Tanner, Kris

Test05 - OptimalF2 - All

Test06 - FindHeights - John. Figure out which options on Find Heights caused a divergent solution

Test07 - BoulderEmission - John. Test if better emission angles allows better representation of the boulder

Test08 - OptimalUltraF2 - Diane, Tanner

Test09 - OrbitBOptimal - OrbitBUltra - Kris, Tanner

Test10 - UltraFeatureF2, All

Test11 - ReferencePeaks, All. Link to Local Tilt results.

NFT Stuff

F3 - Sensitivity Tests

F3 center of figures

F3 Test Procedure

How To - F3 Test Procedure

TestF3A - Baseline (Eric)

TestF3B - Number of Images (Tanner)

TestF3C - Quality of Observing Conditions (Tanner)

TestF3D - LIDAR

TestF3E - Limbs (Kris)

TestF3F - Photometric Function (Diane) - TestF3F - Results and Test F3F3 - Analysis

TestF3G - Navigation Error (Diane) - TestF3G - Results

TestF3H - Latitude (John)

Other test that might be useful

Add noise into the maplet, and see if the good parts remain and the poor parts go away

Surface with simple craters of the same size

Features with specific slopes to evaluate how steep SPC can go

Projects

Fourier transform - Kris, Diane

Mambo_5 - Kris. Polar plots to describe quality of observations

DirtySumfiles - Kris. Creates SUMFILES that can be used with creator_mg and creator_grid to make images at a specific spacecraft az/zenith and sun az/zenith

Whatcamacallit_11 - Tanner.

Tool to show how much maplets shift in 3D space to a truth model

When to Backup

Make the following aliases

alias doneStep='rm -r step*'alias murphy='rsync -hapvP LMKFILES/ ../back-landmarks'

Calibration -- When you are done with a tiling procedures and the needed iterations, you will ensure your logs are up to date and statistics computed, then run rsync to backup the directory.

Also, remove the old statistics directories (step75-a)

cd ..rsync -hapvP --exclude=IMAGEFILES Bennu /Volumes/Share/Shared/SPC-share/<yourid>/2015-07-01-Apch-75cmcd BennudoneStep

For each step (tiling and iteration), you will want to run statistics and copy the needed output into a directory (step75-a).

Make a temporary backup of only the landmarks files (LMKFILES/)

This will over write the previous ones, but that's okay because this is only for your use if you mess up some of them on the next step.

rsync -hapvP LMKFILES/ ../back-landmarks

Make an alias for this

mkdir step75-amove bunch of stuff into step75-amurphy

File Structure

Many things are kept on ormacsrv1.lpl.arizona.edu

Official testing workspace

/SPC_Test

/SPC_Test/F1a -- Dr. Gaskell's test

/SPC_Test/F1b -- Dr. Palmer's test

/SPC_Test/shape3 -- this has the official images needed for the test (only those from Freespace).

PICTLIST.TXT-App -- this has PICTLIST.TXT for each mission phase.

Do a symbolic link to it

PICTLIST.TXT-App.PS -- this has PICTLIST.TXT for each mission phase.

Do a symbolic link to it

PICTLIST.TXT-App.PS.DS -- this has PICTLIST.TXT for each mission phase.

Do a symbolic link to it

PICTLIST.TXT-App.PS.DS.OB -- this has PICTLIST.TXT for each mission phase.

Do a symbolic link to it

mapConf -- Stores the BIGMAP input files to form them. There is a "truth" directory that stores the definitions used to form the truth version (that start with a T)

localbin -- executables that can't be placed in /usr/local/bin

altwg-date-os/bin -- java programs that do AltWG processing, such as CompareOBJ, ICQ2PLT, Maplet2FITS and FITS2OBJ

<working>/support -- Scripts, input files and other files common to all

<working>/lsupport -- Input files unique to each user (project) such as custom <bigmap>.in files

Support and backup data

/Volumes/Share/Shared/SPC-share/SubComp -- Results from the previous System SubComponent Test

/Volumes/Share/Shared/SPC-share/Component -- Results from the previous System Component Test

/Volumes/Share/Shared/SPC-share/F1b -- Saved checkpoints from the F1b test

/Volumes/Share/Shared/SPC-share/shape3-original -- The Freespace source tar.gz files

/Volumes/Share/Shared/SPC-share/truth-bigmaps -- Working directory that has the 5cm (Q=550) BIGMAPS that is Shape3.7

/Volumes/Share/Shared/SPC-share/bennu-image-generate -- Working directory that has the 7000 5cm (tiny) MAPLETS, Shape3.4

/Volumes/Share/Shared/SPC-share/kdrozd -- Backup directories for their tests

/Volumes/Share/Shared/SPC-share/tcampb -- Backup directories for their tests

/Volumes/Share/Shared/SPC-share/jweirch -- Backup directories for their tests

README for major directories

For each top directory in SPC-share and /SPC_Test we need a README that describes the following

README

Purpose of the directory

Major subdirectories and their function

Who created it

Log

Date

What changes were made

Date

More changes

etc.

Test Log Files

For each major step (such as a sequence of tiling and iterations), please create a log file in the working directory. When you start a tiling sequence, update it to the current info testLog.txt

Date

Who is running the test

Test Number/Subtest

Test Name

What is the goal of the test

Log

Date

Major procedures or techniques

Names of BIGMAPs created

Parameters used for tiling or other actions

Seed file used for make_script*.seed and changes to that file

Problems noted and solutions used

Locations for Testing/Shape3

This just lists what we are using for easy reference.

Title	Latitude	Longitude	Feature
TAG 1:	-8.027	262.768W	TAG
TAG 2:	-10.232	334.156W	TAG
TAG 3:	+42.525	114.719W	TAG
Region 1:	-30.000	220.000W	Smooth
Region 2:	-7.000	270.000W	Smooth - Not used
Region 3:	+44.000	199.000W	Smooth
Region 4:	-53.000	59.000W	Smooth
Region 5:	+3.000	41.000W	Smooth
Region 6:	+0.000	301.000W	Rough - Not used
Region 7:	+0.000	335.000W	Rough - Not used
Region 8:	+0.069	319.800W	Rough
Region 9:	+0.000	140.000W	Rough
Boulder 1:	+30.597	190.232W	2.77m
Boulder 2:	-33.488	40.817W	4.07m
Boulder 3:	+18.459	222.335W	8.24m
Boulder 4:	TBD
Boulder 5:	TBD

Bigmap Names

These are some names of the bigmaps that will be used during testing. Truth Shape

TTAG15 - Truth TAG site1, GSD 5cm and 1001x1001 (50x50m)

TTAG25 - Truth TAG site2, GSD 5cm and 1001x1001 (50x50m)

TTAG25 - Truth TAG site3, GSD 5cm and 1001x1001 (50x50m)

TTAG10 - Truth TAG site1, GSD 10cm and 1001x1001 (100x100m)

T15-2K - Truth TAG site1, GSD 5cm and 2001x2001 (100x100m)

T12-5K - Truth TAG site1, GSD 2cm and 5001x5001 (100x100m)

TREG01 - Region 1, GSD 5cm and 1001x1001 (50x50m)

etc.

TEST01 to 7 - Truth TAG site1, GSD of 5cm with different parameters for each.

1-5 are different sizes while 6 and 7 have a slightly different starting location (a few hundredths of a degree -- a few meters)

TJW003 - Boulder 2, GSD 5cm and 1001x1001 (50x50m)

TJW004 - Boulder 1, GSD 5cm and 1001x1001 (50x50m)

TJW005 - Boulder 3, GSD 5cm and 1001x1001 (50x50m)

The names of the model are similar, except the T (for truth) is replaced with M (for model)

MTAG15 - Truth TAG site1, GSD 5cm and 1001x1001 (50x50m)

MTAG25 - Truth TAG site2, GSD 5cm and 1001x1001 (50x50m)

MTAG25 - Truth TAG site3, GSD 5cm and 1001x1001 (50x50m)

MREG01 - Region 1, GSD 5cm and 1001x1001 (50x50m)

MJW003 (or BJW003) - Boulder 2, GSD 5cm and 1001x1001 (50x50m)

MJW004 (or BJW004)- Boulder 1, GSD 5cm and 1001x1001 (50x50m)

MJW005 (or BJW005)- Boulder 3, GSD 5cm and 1001x1001 (50x50m)

Other -- These names don't conflict with the standards of SPC.

TJW001 - Truth bigmaps for John

TTC### - Truth bigmaps for Tanner

TKD### - Truth bigmaps for Kirs

TEP### - Truth bigmaps for Eric

MJW001 - Working bigmaps for John

MTC### - Working bigmaps for Tanner

MKD### - Working bigmaps for Kirs

MEP### - Working bigmaps for Eric

Source bigmaps (the truth that made up the truth)

*The original maplets are stored in /Volumes/Share/Shared/BENNUV3 *The Shape3.7 bigmaps come from /Volumes/Share/Shared/Eric_Bob

A working copy is in /Volumes/Share/Shared/SPC-share/truth-bigmaps

We ran about 1 degree bins (Q=550 at 5cm)

ZS0101

ZS####

ZN####

*The Shape3.8 bigmaps are in /Volumes/Share/Shared/Eric_Bob

B00001

B#####

Naming Scheme for Boulder Maplets

Only 6 characters can be used for the naming of maplets because Bob says so.