SETUP

F3CBLOCK-1A - Clean Setup

F3CBLOCK-1B - Test Setup

TEST

20cm

F3CBLOCK-2A - Tile 20cm

F3CBLOCK-2B - Fix landmarks

F3CBLOCK-3A - Iterate*

F3CBLOCK-3B - Fix Correlation*

10cm

F3CBLOCK-4A - Tile 10cm

F3CBLOCK-4B - Fix landmarks

F3CBLOCK-5A - Iterate*

F3CBLOCK-5B - Fix Correlation*

F3CBLOCK-6 - Fix Imaged

F3CBLOCK-7 - Fix Fitted

F3CBLOCK-8 - Geometry

F3CBLOCK-9A - Iterate*

F3CBLOCK-9B - Fix Correlation*

5cm

F3CBLOCK-10A - Tile 5cm

F3CBLOCK-10B - Fix landmarks

F3CBLOCK-11A - Iterate*

F3CBLOCK-11B - Fix Correlation*

F3CBLOCK-12 - Fix Imaged

F3CBLOCK-13 - Fix Fitted

F3CBLOCK-14 - Geometry

F3CBLOCK-15A - Iterate*

F3CBLOCK-15B - Fix Correlation*

F3CBLOCK-16 - Fix Imaged (IF NECESSARY)

F3CBLOCK-17 - Fix Fitted (IF NECESSARY)

F3CBLOCK-18 - Fix Residuals**

F3CBLOCK-19A - Iterate*,**

F3CBLOCK-19B - Fix Correlation*,**

F3CBLOCK-20 - Fix Holes (Requires repeat of steps 11-19 if any holes are found)

F3CBLOCK-21 - Evaluation

* Run recursively until maplets are "correlated". See Processing States

** Run recursively until maplets are "correlated" and "residualed". See Processing States