Test 11 S/T/U with Overlaps - Unsuitable Viewing Condition Images

The original image suite plan comprised images with the following viewing conditions:

Name	Sun	S/C Az	S/C Zenith	Number of Images	Eliminated Images
Test11S	45, 0, -45	every 45	0, 30, 60	96	16/32 of the 60deg emission angle images
Test11T	45, 0, -45	every 45	0, 20, 40, 60, 80	160	16/32 of the 60deg emission angles images, 32/32 of the 80deg emission angle images
Test11U	45, 0, -45	every 45	0, 14, 30, 45, 60, 75	192	16/32 of the 60deg emission angles images, 32/32 of the 75deg emission angle images

However a number of the viewing conditions proved unsuitable for photoclinometry:

18 images were eliminated due to zero phase angle - Lithos could not resolve the template for these images;

174 images were eliminated due to emission angles >=60deg - the images were automatically eliminated via the t11-10.seed and t11-05.seedn files; inspection of the images (example included below) confirms them to be unsuitable for photoclinometry.

Example Images and Associated Template:

phase angle = 0:

emission angle = 60deg, incidence = 0, 45deg:

emission angle = 70deg, incidence = 0, 45deg:

emission angle = 75deg, incidence = 0, 45deg:

emission angle = 80deg, incidence = 0, 45deg: