Test_Files

Overview

6.4 This will solve for the spacecraft's position and pointing based upon the landmarks (control points)

1 - updates the landmark's pointing vector to be othogonal to the surface

2 - Updates spacecraft position

ALWAYS backup the data before running geometry

Input

/usr/local/bin/geometry12030

Log

Output

List of files:

Bob notes

1 2 0 iterates

1 - landmark vectors (same as lithos, option V)

2 - camera pointing, scobj